AUDIO_SET_VOL

Description

> Set the AudioOut volume configuration. Check the device specification is needed before use this command. Only audio device supports this URL.

Input Argument

> 0~100

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> AUDIO_SET_VOL='84'

- Write Operation

> OK: AUDIO_SET_VOL='84'
> or
> ERROR: AUDIO_SET_VOL='84'

Applicability

- EPL Decoder Devices

Status

> Valid

See Also

> AUDIO_MIC_BOOST

Example

- Read Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&AUDIO_SET_VOL

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&AUDIO_SET_VOL=84

Back to

> HOME, URL CGI