LOGIN

Description

> Login the device and get the level of this logon. Currently, there are two levels for logon user. They are root and user levels. In root level, all features are available. In user level, the feature is very limited.

> The account name and password are given within this URL but not as the input argument. For example, this URL was entered as

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&LOGIN

> The account name and password are carried in this URL. The device will response this logon after it checks this user account information.

> The error message will be returned if the account name or password is incorrect.

Input Argument

> None

Attribute

- Read Only
- Not On-Fly

Return of Message

> If root level logon:
> LOGIN='1'
> If user level logon:
> LOGIN='2'
> If the account name or password is incorrect
> ERROR: bad account/password

Applicability

- EPL Platform : All Encoder Devices
- PlatfotmT : All Encoder Devices

Status

> Valid

See Also

> ACCOUNT, ACCOUNT_ROOT_NAME, ACCOUNT_ROOT_PASSWORD, ACCOUNT_USER_NAME_N, ACCOUNT_USER_PASSWORD_N, ACCOUNT_USER_N

Example

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&LOGIN
> or
> http://ip:port/cgi-bin/cmd/system?LOGIN

Back to

> HOME, SYSTEM CGI