SWITCH

Description

> Force the decoder to move to channel 1 encoder. This URL is only available in WPL Decoder Devices.

Input Argument

> None

Attribute

- Write Only in WPL Decoders
- On-Fly

Return of Message

> None

Applicability

- WPL Decoder Devices

Status

> Valid

See Also

> CHxx_VIDEO_CONNECT, CHxx_VIDEO_VARFPS, CHxx_VIDEO_STREAM, CHxx_VIDEO_AUDIO, CHxx_VIDEO_CONTROL, CHxx_VIDEO_USERNAME, CHxx_VIDEO_PASSWORD, CHxx_PORT_STREAM, CHxx_PORT_CONTROL, CHxx_PORT_MULTICAST, CHxx_PORT_RTP, CHxx_PORT_HTTP, CHxx_SOURCE_TYPE, CHxx_QUAD_CHANNEL, CHxx_CHANNEL, CHxx_TIME, VIDEO_VARFPS

Example

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&SWITCH

Back to

> HOME, URL CGI