HOST

Description

> Get or all main settings on the devices. These settings include

> LAN_HOSTNAME, LANGUAGE, LAN_IP, LAN_HOSTNAME, BAUDRATE, UARTSETTING, OSD_X, OSD_Y, VIDEO_TV, VIDEO_OSD, VOL_AUDIOOUT and VOL_AUDIOIN.

Input Argument

> None

Attribute

- Read Only

Return of Message

> LAN_HOSTNAME='Test'
> LANGUAGE='0'
> LAN_IP='100.100.100.1'
> LAN_NETMASK='255.255.255.0'
> BAUDRATE='9600'
> UARTSETTING='1'
> OSD_X=''
> OSD_Y='50'
> VIDEO_TV='PAL'
> VIDEO_OSD=''
> VOL_AUDIOOUT=''
> VOL_AUDIOIN='2'

Applicability

- WPL Decoder Devices

Status

> Valid

See Also

> LAN_HOSTNAME, LANGUAGE, LAN_IP, LAN_HOSTNAME, BAUDRATE, UARTSETTING, OSD_X, OSD_Y, VIDEO_TV, VIDEO_OSD, VOL_AUDIOOUT and VOL_AUDIOIN

Example

- Read Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&HOST

Back to

> HOME, URL CGI