PORT_SEARCH1_2

PORT_HOST_SEARCH_1, PORT_HOST_SEARCH_2

Description

> Get or Set device search server port numbers. We provide some utilities like IPUtility to find all our devices in the intranet through these UDP search ports.

> When write, the port number will be checked if it was used from other applications.

Input Argument

> UDP port number, 1~65535

Attribute

- Write Only in WPL Decoder Devices
- Readable and Writable in EPL Decoder Devices
- On-Fly (except WPL Decoder Devices)

Return of Message

> In WPL Decoder Devices

> - None

> In EPL Decoder Devices

> - Read Operation

> > PORT_HOST_SEARCH_1='6005'
> > PORT_HOST_SEARCH_2='6006'

> - Write Operation

> > OK: PORT_HOST_SEARCH_1='6005'
> > OK: PORT_HOST_SEARCH_2='6006'
> > or
> > ERROR: PORT_HOST_SEARCH_1='6005'
> > ERROR: PORT_HOST_SEARCH_2='6006'

Applicability

- WPL Decoder Devices
- EPL Decoder Devices

Status

> VALID

See Also

> PORT, PORT_HTTP

Example

- Read Operation (Only in EPL Decoder Devices)

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&PORT_HOST_SEARCH_1
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&PORT_HOST_SEARCH_2

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&PORT_HOST_SEARCH_1=6005
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&PORT_HOST_SEARCH_2=6006

Back to

> HOME, URL CGI