SYSTEM_PROPERTY

Description

> Get the device system property.

Input Argument

> None

Attribute

- Read Only

Return of Message

> SYSTEM='E'
> TYPE='A'
> NO_OF_CHANNEL='01'
> MULTIPLEXING='X'
> NO_OF_AUDIO_WAYS='2'
> AUDIO_TYPE='PCM'
> MOTION_TYPE='0'
> PROTOCOL_TYPE='2'

> Description of System Property Message

> - SYSTEM

> > E: Standalone device
> > A: PC device or Add-on card for PC

> - TYPE

> > A: Video Encoder device
> > B: Video Decoder device

> - NO_OF_CHANNEL

> > 1: not used. fix to 1 always

> - MULTIPLEXING

> > X: it is not a multiplexing device
> > Q: it is a QUAD encoder device
> > R: it is a Rckmount encoder device
> > B: it is a blade encoder device
> > Note that all devices except the QUAD encoder use MULTIPLEXING='X' now

> - NO_OF_AUDIO_WAYS

> > 0: It has no Audio.
> > 1: It has one-way audio (MIC/Line In enabled device)
> > 2: It has two-way audio (MIC/Line In/Audio Out enabled device)

> - AUDIO_TYPE

> > PCM: PCM Audio format

> - MOTION_TYPE

> > 0: 1CH Motion Detection
> > 1: QUAD Channel Motion Detection

> - PROTOCOL_TYPE

> > 1: TCP1.0 protocol
> > 2. TCP2.0 protocol

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatfotmT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> SYSTEM_INFO

Example

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&SYSTEM_PROPERTY
> or
> http://ip:port/cgi-bin/cmd/system?SYSTEM_PROPERTY

Back to

> HOME, SYSTEM CGI