TITLE_NAME

Description

> Get or Set video title name in every channel.

> The CHANNEL=n command has to be set before this URL command. The format of the URL is

> http://ip:port/cgi-bin/quad?USER=Admin&PWD=123456&CHANNEL=n&TITLE_NAME=m
> where
> n is the channel ID started from 1 (Channel 1) and the range is from 1~4.
> m is the title name of the channel. It has be shorter than 8 bytes and could be A~Z, a~z and 0~9 characters. Characters after the 8th character will be removed before set to the device.

Input Argument

> n: character string (< 8bytes) in A~Z, a~z and 0~9.

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> CHANNEL='1'
> TITLE_NAME='CAMERA 1'

- Write Operation

> CHANNEL='1'
> TITLE_NAME='CAMERA 1'
> or
> ERROR: CHANNEL Value Failed (if CHANNEL is out of range)

Applicability

- WPL Platform : QUAD Encoder Only

Status

> Valid

See Also

> OSD_ENABLED

Example

- Read Operation

> http://ip:port/cgi-bin/quad?USER=Admin&PWD=123456&CHANNEL=1&TITLE_NAME

- Write Operation

> http://ip:port/cgi-bin/quad?USER=Admin&PWD=123456&CHANNEL=1&TITLE_NAME='CAMERA 1'

Back to

> HOME, QUAD CGI