ACCOUNT_ROOT_NAME_PASSWORD

ACCOUNT_ROOT_NAME, ACCOUNT_ROOT_PASSWORD

Description

> Get or Set root-level account name and password. Only root has authorized to execute this command.

> Only the root-level account could have right to get or set all settings in the device. The user-level account could get the video and audio stream and some system information only.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, this URL is read-only command and the Router's root ACCOUNT settings will be returned.

Input Argument

> Character string (<32 bytes for name and < 64 bytes for password)

Attribute

- Readable and Writable (except all video servers in Multi-Channel Encoder)
- On-Fly (except all devices in WPL Platform and Multi-Channel Encoder)

Return of Message

- Read Operation

> ACCOUNT_ROOT_NAME='aaaa'
> ACCOUNT_ROOT_PASSWORD='111111'

- Write Operation

> OK: ACCOUNT_ROOT_NAME='aaaa'
> OK: ACCOUNT_ROOT_PASSWORD='111111'
> or
> ERROR: ACCOUNT_ROOT_NAME='aaaa'
> ERROR: ACCOUNT_ROOT_PASSWORD='111111'

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatformT : All Devices
- Multi-Channel Encoder : All Devices

Status

> This URL will be obsolete and replaced by ACCOUNT_ROOT

See Also

> ACCOUNT, ACCONT_ROOT, ACCOUNT_USER_NAME_N, ACCOUNT_USER_PASSWORD_N, ACCOUNT_USER_N

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&ACCOUNT_ROOT_NAME
> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&ACCOUNT_ROOT_PASSWORD
> or
> http://ip:port/cgi-bin/cmd/system?ACCOUNT_ROOT_NAME
> http://ip:port/cgi-bin/cmd/system?ACCOUNT_ROOT_PASSWORD

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&ACCOUNT_ROOT_NAME=aaaa
> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&ACCOUNT_ROOT_PASSWORD=111111
> or
> http://ip:port/cgi-bin/cmd/system?ACCOUNT_ROOT_NAME=aaaa
> http://ip:port/cgi-bin/cmd/system?ACCOUNT_ROOT_PASSWORD=111111

Back to

> HOME, SYSTEM CGI