ACCOUNT

Description

> Get device ACCOUNT which it has one root-level account and 10 user-level accounts configuration. Only root has authorized to execute this command.

> Only the root-level account could have right to get or set all settings in the device. The user-level account could get the video and audio stream and some system information only.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, the command is read-only and Router's ACCOUNT configurations will be returned.

Input Argument

> None

Attribute

- Read Only

Return of Message

> ACCOUNT_ROOT_NAME='aaaa'
> ACCOUNT_ROOT_PASSWORD='111111'
> ACCONT_USER_NAME_1=''
> ACCONT_USER_PASSWORD_1=''
> ACCONT_USER_NAME_2=''
> ACCONT_USER_PASSWORD_2=''
> ACCONT_USER_NAME_3=''
> ACCONT_USER_PASSWORD_3=''
> ACCONT_USER_NAME_4=''
> ACCONT_USER_PASSWORD_4=''
> ACCONT_USER_NAME_5=''
> ACCONT_USER_PASSWORD_5=''
> ACCONT_USER_NAME_6=''
> ACCONT_USER_PASSWORD_6=''
> ACCONT_USER_NAME_7=''
> ACCONT_USER_PASSWORD_7=''
> ACCONT_USER_NAME_8=''
> ACCONT_USER_PASSWORD_8=''
> ACCONT_USER_NAME_9=''
> ACCONT_USER_PASSWORD_9=''
> ACCONT_USER_NAME_10=''
> ACCONT_USER_PASSWORD_10=''

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatfotmT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> ACCOUNT_ROOT_NAME, ACCOUNT_ROOT_PASSWORD, ACCONT_ROOT, ACCOUNT_USER_NAME_N, ACCOUNT_USER_PASSWORD_N, ACCOUNT_USER_N

Example

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&ACCOUNT
> or
> http://ip:port/cgi-bin/cmd/system?ACCOUNT

Back to

> HOME, SYSTEM CGI