LENS_COMPENSATION

Description

> In camera, it might have some calibration of the default lens. If the user change the lens, it might do not need to do the calibration. In this case, user needs to disable this function.

> The error message will be returned if the encoder does not support this URL.

Input Argument

> 0: Not Calibrate the lens, 1: Calibrate the lens

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: LENS_COMPENSATION='1'

- Write Operation

> OK:LENS_COMPENSATION='1'
> or
> ERROR: LENS_COMPENSATION='1'

Applicability

- EPL Platform : All Encoders with sensor MT9V135 or MT9M131
- PlatfotmT : All Encoders with sensor MT9M131

Status

> Valid

See Also

> VIDEO_MIRROR_MODE, VIDEO_FLIP_MODE, DAY_GAIN_THD

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&LENS_COMPENSATION
> or
> http://ip:port/cgi-bin/cmd/encoder? LENS_COMPENSATION

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&LENS_COMPENSATION=1
> or
> http://ip:port/cgi-bin/cmd/encoder? LENS_COMPENSATION=1

Back to

> HOME, ENCODER CGI