V2_STREAMING_TYPE

Description

> Get the device's video/audio streaming protocol to connect to encoders.

> There are two video/audio streaming protocols we offered. One is TCP 1.0 which is out of fashion and available in all 1CH, 2CH and QUAD Encoders and Decoder in WPL Platform. The other one is TCP 2.0 which is most use. In all EPL, PlatformT and Multi-Channel devices, only this protocol is available.

Input Argument

> None

Attribute

- Read Only
- Not On-Fly

Return of Message

- Read Operation

> V2_STREAMING_TYPE='2'

Applicability

- EPL Encoder Devices

Status

> Valid

See Also

> PROTOCOL_VERSION

Example

- Read Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&V2_STREAMING_TYPE

Back to

> HOME, URL CGI