WAN_PPPOE

WAN_PPPOE_USERNAME, WAN_PPPOE_PASSWORD

Description

> Get or set the PPPoE configuration on WAN port. These Settings are only valid if only if the WAN_TYPE is PPPoE. The input argument string length will be checked before apply it.

> In EPL decoder, this URL is same as the WAN_PPPOE_USERNAME and WAN_PPPOE_PASSWORD in the SYSTEM CGI but only Type1 URL command is supported.

> Therefore, the WAN_PPPOE_USERNAME and WAN_PPPOE_PASSWORD URLs in WPL decoders are only addressed in this page.

Input Argument

> Character strings (< 64 Bytes)

Attribute

- Write Only
- Not On-Fly

Return of Message

> None

Applicability

- WPL Decoder Devices
- EPL Decoder Devices (refer to WAN_PPPOE_USERNAMEand WAN_PPPOE_PASSWORD in the SYSTEM CGI)

Status

> Valid

See Also

> WAN, WAN_TYPE, WAN_IP, WAN_NETMASK, WAN_GATEWAY

Example

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&WAN_PPPOE_USERAME=''
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&WAN_PPPOE_PASSWORD=''

Back to

> HOME, URL CGI, SYSTEM CGI

¡@