AUDIO_OUT_VOLUME

AUDIO_OUT_LEVEL

Description

> Get or Set the AudioOut level configuration. Check the device specification is needed before use this command. Only audio device supports this URL.

> This URL is only for WPL Decoder Devices because their AudioOut Volume range is very different from EPL and PlatformT Decoder devices. In the WPL Decoder Devices, there are four levels of the AudioOut, MUTE, SMALL, MIDDLE and HIGH.

Input Argument

> MUTE, SMALL, MIDDLE or HIGH

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> AUDIO_OUT_LEVEL='HIGH'

- Write Operation

> OK: AUDIO_OUT_LEVEL='HIGH'
> or
> ERROR: AUDIO_OUT_LEVEL='HIGH'

Applicability

- WPL Decoder Devices (version V2.05.01 and later)

Status

> Valid

See Also

> AUDIO_OUT_VOLUME

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&AUDIO_OUT_LEVEL
> or
> http://ip:port/cgi-bin/cmd/system?AUDIO_OUT_LEVEL

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&AUDIO_OUT_LEVELE=HIGH
> or
> http://ip:port/cgi-bin/cmd/system?AUDIO_OUT_LEVELE=HIGH

Back to

> HOME, SYSTEM CGI