V2_STRAM_PROTOCOL

V2_STREAMING_TYPE, PROTOCOL_TYPE

Description

> Get or Set the device's video/audio streaming protocol.

> There are two video/audio streaming protocols we offered. One is TCP 1.0 which is out of fashion and available in all 1CH, 2CH and QUAD Encoders and Decoder in WPL Platform. The other one is TCP 2.0 which is most use. In all EPL, PlatformT and Multi-Channel devices, only this protocol is available.

> In all WPL Encoder devices, the V2_STREAMING_TYPE is READ/WRITE command and PROTOCOL_TYPE is READ Only command.

> In all EPL, PlatformT and Multi-Channel Encoder devices, these two commands are read only and 2 is returned always.

Input Argument

> 1 : TCP 1.0
> 2 : TCP 2.0

Attribute

- Readable and Writable
- Not On-Fly

Return of Message

- Read Operation

> V2_STREAMING_TYPE='2' or PROTOCOL_TYPE='2'

- Write Operation

> OK: V2_STREAMING_TYPE='2'
> or
> ERROR: V2_STREAMING_TYPE='2'

Applicability

- WPL Platform : All Encoder Devices
- EPL Platform : All Encoder Devices
- PlatformT : All Encoder Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> V2_STREAMING_METHOD

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_STREAMING_TYPE
> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&PROTOCOL_TYPE
> or
> http://ip:port/cgi-bin/cmd/system?V2_STREAMING_TYPE
> http://ip:port/cgi-bin/cmd/system?PROTOCOL_TYPE

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_STREAMING_TYPE=2
> or
> http://ip:port/cgi-bin/cmd/system?V2_STREAMING_TYPE=2

Back to

> HOME, SYSTEM CGI