OSD

OSD_DATE_TIME, OSD_SERVER_IP, OSD_CAMERA_NAME, OSD_LOCAL_IP, OSD_MOTION_DETECT, OSD_STATUS

Description

> Enable or Disable to show the specific information of the encoder or decoder on the OSD.

> The Decoder could show some information of Encoder or itself on the TV screen. The information is listed below.

> Information on the OSD | Related URL
> Date and Time information of the encoder | OSD_DATE_TIME, OSD_DATE_FORMAT
> The IP addresses of the encoder | OSD_SERVER_IP
> The camera name of the encoder | OSD_CAMERA_NAME
> The IP addresses of the Decoder | OSD_LOCAL_IP
> The Motion Trigger form the encoder | OSD_MOTION_DETECT
> The DI Trigger from the Encoder | OSD_STATUS

> These URLs in the above table, control if the associated information could be shown in the TV screen or not. Please refer these URLs for further details.

> The input argument of these URL is "1", the associated information will be shown on the TV screen. Otherwise, the associated information will be shown.

> Note for OSD_STATUS

> > The DI Trigger on the Decoder is shown on the OSD if only if the DI1 and DI2 were triggered by the encoder at the same time.

Input Argument

> n (1: Enable, 0: Disable)

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OSD_DATE_TIME='1'
> OSD_SERVER_IP='1'
> OSD_CAMERA_NAME='1'
> OSD_LOCAL_IP='1'
> OSD_MOTION_DETECT='1'
> OSD_STATUS='1'

- Write Operation

> OK: OSD_DATE_TIME='1'
> OK: OSD_SERVER_IP='1'
> OK: OSD_CAMERA_NAME='1'
> OK: OSD_LOCAL_IP='1'
> OK: OSD_MOTION_DETECT='1'
> OK: OSD_STATUS='1'
> or
> ERROR: OSD_DATE_TIME='1'
> ERROR: OSD_SERVER_IP='1'
> ERROR: OSD_CAMERA_NAME='1'
> ERROR: OSD_LOCAL_IP='1'
> ERROR: OSD_MOTION_DETECT='1'
> ERROR: OSD_STATUS='1'

Applicability

- EPL Decoder Devices

Status

> Valid

See Also

> OSD, OSD_X, OSD_Y, OSD_DATE_FORMAT

Example

- Read Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_DATE_TIME
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_SERVER_IP
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_CAMERA_NAME
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_LOCAL_IP
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_MOTION_DETECT
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_STATUS

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_DATE_TIME='1'
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_SERVER_IP='1'
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_CAMERA_NAME='1'
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_LOCAL_IP='1'
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_MOTION_DETECT='1'
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&OSD_STATUS='1'

Back to

> HOME, URL CGI