ACCOUNT_USER_NAME_PASSWORD

ACCOUNT_USER_NAME_N, ACCOUNT_USER_PASSWORD_N

where N is the user-level index started from 1.

Description

> Get or Set user-level account name and password. Only root and the same user index account have authorized to execute this command.

> When write, the account name has not be the same as the root account name.

> Only the root-level account could have right to get or set all settings in the device. The user-level account could get the video and audio stream and some system information only.

> Because there are 10 user-level accounts in the device, the last character, N, in these command indicates the user index of the user-level account and its range is in 1~10.

> In EPL decoder, these URLs are same as the ACCOUNT_USER_NAME_N and ACCOUNT_USER_PASSWORD_N in the SYSTEM CGI but only Type1 URL command is supported.

> Therefore, the ACCOUNT_USER_NAME_N and ACCOUNT_USER_PASSWORD_N URL in WPL decoders are only addressed in this page.

Input Argument

> Character string (<32 bytes for name and < 64 bytes for password)

Attribute

- Write Only
- Not On-Fly

Return of Message

> None

Applicability

- WPL Decoder Devices
- EPL Decoder Devices

Status

> Valid

See Also

> ACCOUNT, ACCOUNT_ROOT_NAME, ACCOUNT_ROOT_PASSWORD

Example

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&ACCOUNT_USER_NAME_N=''
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&ACCOUNT_USER_PASSWORD_N=''

Back to

> HOME, URL_CGI, SYSTEM CGI