REBOOT

Description

> Reboot the device. The runtime configuration might be lost if it has not be saved into flash after this URL was executed

Input Argument

> None

Attribute

- Not On-Fly

Return of Message

> Always return OK

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatfotmT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> FACTORY_DEFUALT, SAVE_REBOOT, SAVE

Example

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&REBOOT
> or
> http://ip:port/cgi-bin/cmd/system?REBOOT

Back to

> HOME, SYSTEM CGI