ACCOUNT_USER

ACCOUNT_USER_N

Description

> Get or Set user index Naccount name and password. Only root and the same user index account have authorized to execute this command.

> When write, the account name has not be the same as the root account name.

> Only the root-level account could have right to get or set all settings in the device. The user-level account could get the video and audio stream and some system information only.

> Because there are 10 user-level accounts in the device, the last character, N, in these command indicates the user index of the user-level account and its range is in 1~10.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, this URL is read-only command and the Router's root ACCOUNT settings will be returned.

Input Argument

> n,m
> where
> n : Character string (<32 bytes) for user index N account name
> m : Character string (< 64 bytes) for user index N account password

Attribute

- Readable and Writable (except all video servers in Multi-Channel Encoder)
- On-Fly (except all devices in Multi-Channel Encoder)

Return of Message

- Read Operation

> ACCOUNT_USER_N=','

- Write Operation

> OK: ACCOUNT_USER_N='user,123'
> or
> ERROR: ACCOUNT_USER_N=','

Applicability

- EPL Platform : All Devices
- PlatformT : All Devices
- Multi-Channel Encoder : All Devices

Status

> This URL is new command for replacing the URL ACCOUNT_USER_NAME_N and ACCOUNT_USER_PASSWORD_N

See Also

> ACCOUNT, ACCOUNT_ROOT_NAME, ACCOUNT_ROOT_PASSWORD, ACCONT_ROOT, ACCOUNT_USER_NAME_N, ACCOUNT_USER_PASSWORD_N

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&ACCOUNT_USER_N
> or
> http://ip:port/cgi-bin/cmd/system?ACCOUNT_USER_N

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&ACCOUNT_USER_N=user,123
> or
> http://ip:port/cgi-bin/cmd/system?ACCOUNT_USER_N=user,123

Back to

> HOME, SYSTEM CGI